1. Choose items you want from the four buttons and click "Send" button. 
2. Enter the corresponding offset value (within -12V and +12V) from the right input box when the Offset is On.
3. Click the "Store" button to save the current working state of PA (the state saved here is only the current working state of PA independently of options on the control panel.) 